**Project Removed**

Madera South High School-updated map

Section A

* 12x26 (312 sq/ft)
* Remove asphalt and pour back with concrete at 6’’ thickness with #4 rebar at 18’’ o.c.
* Dowel into existing concrete every 2 feet with #4 rebar.
* Rebar is to penetrate 8 inches into existing concrete and protrude 18 inches.
* Restripe white 12” wide by 12’ long line and “STOP” using 8-foot font.

Section B

* 12x26 (312 sq/ft)
* Remove asphalt and pour back with concrete at 6’’ thickness with #4 rebar at 18’’ o.c.
* Dowel into existing concrete every 2 feet with #4 rebar.
* Rebar is to penetrate 8 inches into existing concrete and protrude 18 inches.
* Restripe white 12” wide by 12’ long line and “STOP” using 8-foot font.



